RF enhancements

To have validation on RF for multiple DN (3 orders) assigned to 1 wavekey. Validate 1 Tote Bin to 1 order. RF screen to prompt error message when picker scan the same Tote Bin ID for a different order (DN) that was previously used to pick for another order under the same wave.

Refer to attachment on the re-arrangement of data fields in RF.