**Putaway logic**

**1.    Modify the putaway logic in RF for non-batch / Batch managed SKU regardless of whether it is serialized**

For putaway,

-       To suggest 1 LP to 1 Loc (one Loc cannot have mulitple LPs of a similar SKU but may contain different SKUs.

- Exceptions:

a) Freezer locations

b) Location flag =”HOLD”

c) Status = “HOLD”

-        Suggest location in following order:

1.    Most recent location in historical records and is empty

2.    Most recent location in historical records and does not contain this SKU

3.    Empty location if point 1 & 2 is not applicable.

**2.    There will also be a need to change the validation logic for RF & WMS move function & WMS transfer movement module.**

RF, WMS move function & WMS transfer movement – to block user from moving different LP of a similar SKU into the same location

Exceptions:

a) Freezer locations

b) Location flag =”HOLD”

c) Status = “HOLD”